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Chassis

Component

Fluid, Lubricant, or Genuine Part

Automatic Transmission

Use only Mopar ZF 8&9 Speed ATF Automatic Transmis-
sion Fluid, or equivalent.

Failure to use the correct fluid may affect the function or
performance of your transmission.

Brake Master Cylinder

We recommend you use Mopar DOT 3 Brake Fluid, SAE
J1703 should be used. If DOT 3, SAE ]J1703 brake fluid is not
available, then DOT 4 is acceptable. Use only recom-
mended brake fluids.
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Maintenance Plan
Required Maintenance Intervals.

Refer to the “Maintenance Plan” in this section for the
required maintenance intervals.

At Every Oil Change Interval As Indicated By Ol
Change Indicator System:

o Change oil and filter

+ Rotate the tires. Rotate at the first sign of irregular
‘wear, even if it occurs before the oil indicator system
turns on

At Every Oil Change Interval As Indicated By Oil
Change Indicator System:

« Tnspect battery and clean and tighten terminals as

required

Inspect brake pads, shoes, rotors, drums, hoses and
park brake

* Inspect engine cooling system protection and hoses

 Inspect exhaust system

« Tnspect engine air cleaner if using in dusty or

off-road conditions
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Additional Inspections
Inspect the CV joints. X X X X X
Inspect front suspension, boot seals. tie rod ends, X X
and replace if necessary. X
Inspect the brake linings, parking brake function. X
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Inspect front accessory drive belt, tensioner, idler pul- X
ley, and replace if necessary.
Additional Maintenance
Replace engine air cleaner filter. X X X X
Replace air conditioning/cabin air filter. X X X X X X
Replace spark plugs — 2.0L Engine™ X
Replace spark plugs — 2.4L & 3.2 Engine™ X
Flush and replace the engine coolant at 10 years or X X
150,000 miles (240,000 km) whichever comes first.
Inspect and replace PCV valve if necessary. X
* The spark plug change interval is mileage based only, AN

yearly intervals do not apply.

© You can be badly injured working on or around a
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Lubricants which do not have both the engine oil certifi-
cation mark and the correct SAE viscosity grade number
should not be used.

Engine Oil Viscosity (SAE Grade) — 3.2L Engine
engine oil or equivalent Pennzoil or
is recommended for all operating temperatures.

This engine oil improves low temperature starting and
vehicle fuel economy. The engine oil filler cap also shows
the recommended engine oil viscosity for your engine. For
information on engine oil filler cap location, refer to

“Engine Compartment” in this section.

Lubricants which do not have both the engine oil certifi-
cation mark and the correct SAE viscosity grade number
should not be used.

Synthetic Engine Oils

You may use synthetic engine oils provided the recom-
mended oil quality requirements are met, and the recom-
‘mended maintenance intervals for ol and filter changes are
followed.

Synthetic engine oils which do not have both the engine oil

certification mark and the correct SAE viscosity grade
number should not be used.

Materials Added To Engine Oil

The manufacturer strongly recommends against the addi-
tion of any additives (other than leak detection dyes) to the
engine oil. Engine oil is an engineered product and its
performance may be impaired by supplemental additives.

Disposing Of Used Engine Oil And Oil Filters

Care should be taken in disposing of used engine oil and
oil filters from your vehicle. Used oil and oil filters,
indiscriminately discarded, can present a problem to the
environment. Contact an authorized dealer, service station
or governmental agency for advice on how and where used
oil and oil filters can be safely discarded in your area.

Engine Oil Filter

The engine oil filter should be replaced with a new filter at
every engine oil change.

Engine Oil Filter Selection

This manufacturer’s engines have afull-flow type dispos-
able oil filter. for replacement. The
quality of replacement filters varies considerably. Only
high quality filters should be used to assure most efficient
service. engine oil filters are high quality oil filters
and are recommended.
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Engine Air Cleaner Filter

Refer to the “Maintenance Plan” in this section for the
proper maintenance intervals.

NOTE: Be sure to follow the “Severe Duty Conditions”
maintenance interval if applicable.

WARNING!

The air induction system (air cleaner, hoses, etc.) can
provide a measure of protection in the case of engine
backfire. Do not remove the air induction system (air
cleaner, hoses, etc.) unless such removal is necessary
for repair or maintenance. Make sure that no one is
near the engine compartment before starting the ve-
hicle with the air induction system (air cleaner, hoses,
etc.) removed. Failure to do so can result in serious
personal injury.

Engine Air Cleaner Filter Selection

The quality of replacement engine air cleaner filters varies

considerably. Only high quality: filters should be used to

assure most efficient service. Mopar  engine air cleaner
filters are a high quality filter and are recommended.

Engine Air Cleaner Filter Inspection and
Replacement

Inspect engine air cleaner filter for dirt and or debris, if you
find evidence of either dirt or debris you should change
your air cleaner filter.

Engine Air Cleaner Filter Removal

1. Remove the screws from the air cleaner cover.
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Air Cleaner Filter Cover

1 — Clean Air Hose Clamp
2 — Screws
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FLUID CAPACITIES

Us. Metric
Fuel (Approximate)
All Engines 15.8 Gallons 60 Liters
Engine Oil With Filter
2.0 Liter Engine (SAE 5W-30, API SN 5 Quarts 4.7 Liters
PLUS Certified)
24 Liter Engine (SAE 0W-20, APT 5.5 Quarts 5.2 Liters
Certified)
3.2 Liter Engine (SAE 5W-20, API 6 Quarts 5.6 Liters
Certified)
Cooling System*
2.0 Liter Engine (Mopar Antifreeze/ 9 Quarts 8.6 Liters
Engine Coolant 10 Year /150,000 Mile
Formula)
24 Liter Engine (Mopar Antifreeze/ 7.2 Quarts 6.8 Liters
Engine Coolant 10 Year/150,000 Mile
Formula)
3.2 Liter Engine (Mopar Antifreeze/. 10 Quarts 95 Liters
Engine Coolant 10 Year /150,000 Mile
Formula)
* Includes heater and coolant recovery bottle filled to MAX level.
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FLUIDS AND LUBRICANTS
Engine

Component

Fluid, Lubricant, or Genuine Part

Engine Coolant

We recommend you use Mopar Antifreeze/Coolant 10 Year/150,000-Mile
Pormmala"OAT=(Organic Additive Technology) or equivalent meeting the

requirements of FCA Standard MS.90032.

Engine Oil - 2.0L Engine

We recommend you use Mopar API SN PLUS Certified SAE 5W-30 Full
Synthetic Engine Ol which meets the requirements of FCA Material Standard
MS-13340. Equivalent full synthetic SAE 5W-30 engine oil can be used if it
meets API SN PLUS Certification. If SN PLUS or equivalent oil is unavailable
then please contact your local dealership for recommendation.

CAUTION!

Failure to use the recommended SN PLUS or equivalent oil can cause
engine damage not covered by the vehicle warranty.

Engine Oil - 24L Engine

We recommend you use SAE OW-20 AP Certified Engine Ofl, meeting the
requirements of FCA Material Standard MS-6395 such as Mopar, Pennzoil,
and Shell Helix. Refer to your engine ol filler cap for correct SAE grade.

Engine Oil - 32L Engine

We recommend you use API Certified SAE 5W-20 Engine Oil, mecting the
requirements of FCA Material Standard MS-6395 such as Mopar, Pennzoil,
and Shell Helix. Refer to your engine oil filler cap for correct SAE grade.

Engine Oil Filter

We recommend you use a Mopar Engine Oil Filter.

Spark Plugs

We recommend you use Mopar Spark Plugs.





